Cable Name: AT-SF1P/CBL04

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  | | --- | | DCJ20-0442SVB-L  CONN.PWR,DC,JACK  2.0MM PIN,LOCK | |  | |  | |  | |  | |  | |  | | DB15 MALE NAZ-15P TCTC-15  *Label* **SWITCH BOX** | AK-1550-6-3,5  CONN,TB,WR,6PIN,(F),  8A,GREEN |  |
|  |
|  |
|  |
|  |
|  |
|  |
| 1 | 2, 5 |  | red |
|  | 3 | 4 | white |
|  | 6 | 5 | white-brown |
|  | DB25 MALE NBZ-25P  TCTC-25  *Label* **PioPort 7-9** |  |  |
|  |  |  |
|  |  |  |
|  | 1 | 1 | Yellow |
|  | 2 | 2 | Yellow-green |
| 2 | 25 | 3, 5 | black |

|  |  |
| --- | --- |
| Length **|**<--------- 100 cm ------>**|** |  |
| **|**<----------180 cm ------------->**|** | |



Please attach a label the with Cable Name and label to the cable